надо быть действительно великим человеком, чтобы суметь устоять даже против здравого смысла

http://golos-dobra.livejournal.com/1130343.html

### надо быть действительно великим человеком, чтобы суметь устоять даже против здравого смысла

Dec. 2nd, 2012
https://aleks-aberdin.livejournal.com/294832.html
Моя бабушка была неграмотной. Некогда ей было учиться грамоте. Но даже она знала, что китайцев на острове Даманском пожгли лазарем. Я пытался объяснить ей, что не лазарем, а лазером, но она только отмахивалась и говорила, что батюшка Михаил, священник нашей церкви, а он по соседству жил через 2 дома, лучше меня знает. Таким было первое известие о боевых возможностях советского лазерного оружия, о котором я уже знал из научной фантастики. А потом была учёба в Краснодаре и дружба с ребятами, учившимися на физфаке, некоторые из которых занимались лазерами, а также выращиванием кристаллов. Вот тогда-то я и узнал, что в Краснодаре есть секретная лаборатория, в которой профессор Бадиков, ученик Рэма Хохлова, выращивает самые большие в мире кристаллы рубина и сапфира. Узнал я и о том, что в этой лаборатории был якобы выращен гигантский монокристалл рубина, из которого впоследствии выточили рубиновый стержень длиной в 84 см для самого мощного в мире лазера и что для одного выстрела требуется энергия всей Красноярской ГЭС. Так это или нет я не знаю и всего лишь пересказываю то, о чём когда-то рассказывал мой друг по прозвищу академик Папица. После этого я много чего слышал и читал про лазеры, даже по ящику про них рассказывали, а предпоследним известием было то, что американцы оснастили "Боинг" боевым лазером, но из этого рая не вышло ни... чего. И вот буквально только что я надыбал информацию о том, что в Эрефии вознамерились возродить программу создания боевых лазарей. Всё бы ничего, но одно то, что их будут ставить на самолётах, как-то напрягает, поскольку делает похожим такое оружие на обычные развесистые понты и распальцовку. Но ещё больше лично меня напрягают такие слова из той статьи, которую, вместе с краткой историей создание лазерного оружия, вы можете прочитать под катом: "Как раз под такие цели в октябре 2012 года по инициативе вице-премьера Дмитрия Рогозина был создан Фонд перспективных исследований (ФПИ). И денег на "высокорискованные научные исследования и разработки" правительство, судя по всему, жалеть не станет." И вот почему. А не идёт ли здесь речь всего лишь об элементарном распиле бюджетных денег?
http://iopscience.iop.org/article/10.1088/2399-6528/aab007/pdf
PUBLISHED
22 March 2018
Widely tunable (2.6–10.4 μm) BaGa4Se7 optical parametric oscillator pumped by a Q-switched Nd:YLiF4 laser
Special Technologies, Ltd, 1/3 Zeljonaja gorka str., 630060 Novosibirsk, Russia
Research Laboratory of Quantum Optics Technology, Novosibirsk State University, 2 Pirogova Str., 630090 Novosibirsk, Russia 3 Institute of Laser Physics SB RAS, Lavrentyev av. 13/3, 630090 Novosibirsk, Russia
Novosibirsk State Technical University, K. Marx av. 20, 630073 Novosibirsk, Russia
High Technologies Laboratory, Kuban State University, 149 Stavropolskaya Str., 350040 Krasnodar, Russia.
School of Science and Technology, Nazarbayev University, 53 Kabanbay Batyr Ave., 010000 Astana, Kazakhstan
Widely tunable optical parametric oscillators are attractive laser sources for mid-infrared (MIR) nonlinear optics applications, because of the scarcity of direct-emitting conventional laser sources in this spectral region (2–20 μm). While oxide-based periodically-poled nonlinear compounds belonging to the ferroelectric crystal family (mainly LiNbO3, LiTaO3 and KTiOPO4) are commercially available, their IR transparency does not exceed 5 microns and therefore they cannot be used for deeper MIR applications. For instance the 8–14 μm range corresponding to one of the atmospheric transparency window is interesting for LIDAR or countermeasure systems while coherent sources in the strongly water-absorbing 6–7 μm range can be used for medical (surgery) applications. More generally tunable coherent MIR laser sources are useful spectroscopic tools to probe rovibrational molecular fingerprints with various applications in trace gas sensing such as environmental monitoring, detection of hazardous species, life science or medical applications such as real-time breath analysis for early disease diagnosis.
Currently very few nonlinear chalcogenide compounds possessing both wide transparency range above
5 μm and large energy bandgap are available. The bandgap wavelength requirement is necessary to avoid two-photon absorption (TPA) when they are pumped with popular 1 μm range solid-state emitting lasers such as Nd3+ lasers or Yb3+ fiber lasers. Only a handful of ternary compounds satisfies the requirement of wide bandgap and extended MIR transparency range, with proven capabilities for down-conversion to the long-wave MIR using 1.064 μm pump optical parametric oscillation (OPO). Among these latter ones — whose use in nanosecond OPOs have been widely proven owing to their commercialization—one can quote the benchmark wurzite-type ternary chalcopyrite AgGaS2 (AGS) belonging to the AIIBIV C2V semiconductor group and, to a lesser extent, the much more limited transparency range ZnGeP2 (ZGP) belonging to the AIBIIIC2VI group. During more than a decade silver gallium sulfide (AgGaS2) has been the only OPO material with the longest demonstrated idler wavelength.
Since the mid 90’s, some novel ternary lithium containing chalcogenides (LiInS2, LiInSe2, LiGaS2, LiGaSe2) produced with large enough single-crystal size have emerged, leading to various nanosecond OPO demonstrations covering the mid-IR despite their rather low nonlinearity compared to ZGP or the difficult-to-grow mercury thiogallate, HgGa2S4 (HGS). The recently re-discovered II–IV–V2 chalcopyrite compound CdSiP2 (CSP) with its high nonlinearity could appear as an alternative to ZGP, however its low bandgap combined with limited MIR transparence (λ=6.5 μm) almost restrict its use to the non-critically phase-matched generation of ∼6 μm radiation when pumped at 1064 nm. Alternative to birefringence phase-matched compounds, orientation-patterned III-IV semi-conductors (orientation-patterned GaAs and GaP) with high nonlinearity have been recently engineered, however their low bandgap energy does not allow 1 μm pumping not only because of TPA but also due to strong absorption resulting in tremendous thermal load. OP-GaAs and OP-GaP require thus pumping above ∼2 microns and have limited aperture (
https://www.spiedigitallibrary.org/conference-proceedings-of-spie/10637/106370U/Status-of-CdSiPsub2-sub-development-for-scaling-mid-infrared-laser/10.1117/12.2306527.short?SSO=1
4 May 2018
Status of CdSiP2 development for scaling mid-infrared laser power
Carl M. Liebig , F. Kenneth Hopkins , Kent L. Averett
Air Force Research Lab. (United States)
Kevin T. Zawilski , Peter G. Schunemann
BAE Systems (United States)
Elizabeth M. Scherrer , Nancy C. Giles , Larry E. Halliburton
Air Force Institute of Technology (United States)
https://nationalinterest.org/blog/buzz/here-come-lasers-dawn-energy-weapons-here-26671
July 24, 2018 Topic: Security Blog Brand: The Buzz Tags: MilitaryWorldTechnologyLaser
Here Come the Lasers: The Dawn of Energy Weapons Is Here
Is it possible the maturation of one advanced technology can be such a disruptive innovation to the point where certain types of warfare begin to look different?
https://www.nextbigfuture.com/2018/08/us-targets-a-megawatt-laser-by-2023-and-then-deployment-in-drones-and-satellites-for-hypersonic-and-icbm-defense.html
August 15, 2018
US targets a megawatt laser by 2023 and then deployment in drones and satellites for hypersonic and ICBM defense
The DARPA High Energy Liquid Laser Area Defense System (HELLADS) fourth phase is a ground-based laser weapon system demonstrator with an approximate average power of 150 kW. One of the goals is to make lasers lighter and more compact. The goal is 5 kg per kW. The High Energy Liquid Laser Area Defence System (HELLADS) will weigh just 750 kilograms and fit into a space about the size of a large refrigerator